|  | about 4C news 4C guide theory applications publications contact |  | user interface | user manual
Data processing and test of goodness of fit After simulation, data processing can be started. Herefore, a file with measurements is read in after prompting. Comparison and test of goodness of fit apply to the generated (or existing) 4C-Output files. A descriptive statistic is calculated for each measurement type and each run, containing simulation value, measurement, residuum and various error measures. A detailed description of the processes and the structure of the output files can be seen here. ###
about 4C | news | 4C guide | theory | applications | publications | contact